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WALL COVERING
PART 1  GENERAL
SECTION INCLUDES
Tackable Wall Panels.
REFERENCE STANDARDS
ASTM B221 - Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles, and Tubes; 2021.
ASTM C208 - Standard Specification for Cellulosic Fiber Insulating Board; 2022.
ASTM E84 - Standard Test Method for Surface Burning Characteristics of Building Materials; 2024.
ASTM F793/F793M - Standard Classification of Wall Coverings and Ceiling Coverings by Use Characteristics; 2025.
SUBMITTALS
Product Data:  Provide manufacturer's data on Tackable Wall Covering. Include Material Safety Data Sheets when applicable.
Shop Drawings: Submit shop drawings for each type of visual display board as specified, including sectional details, trim, face and core materials, dimensions, joint locations, and any special anchor details. ​, special anchor details​.
Color Samples: Provide a complete set of color swatches showcasing the manufacturer's full selection of colors and finishes for Tackable Wall Covering.
Product Samples: ​Two​, [10" by 10"] inches [254 by 254] mm in size illustrating materials and finish, color and texture of ​tackable surfaces​.
Manufacturer's printed installation instructions.
QUALITY ASSURANCE
Manufacturer Qualifications: Company specializing in manufacturing the products specified in this section with minimum ​​20​​ years​​ documented​​ experience.
WARRANTY
Provide the manufacturer's standard five-year warranty workmanship, confirming that, with proper usage, maintenance, and installation according to the manufacturer's guidelines, the tackable panels are guaranteed for five-year from the date of substantial completion.
Warranty does not cover labor, removal or reinstallation of Tack Wall Panels.
PART 2  PRODUCTS
MANUFACTURERS
Tackable Wall Panels
Nelson Adams NACO
Address: 420 S. E St. San Bernardino CA 92401
P: (877) 810-4080
Web Page: https://nelsonadamsnaco.com
TACKABLE WALL SURFACING
Tackable Wall Panels: Tackwall panels substrate construction consist of standard vinyl on 1/2" or 3/8''  fiberboard with vinyl wrapped plastic J-trim.
Material Facing: [ Fabric ][ Vinyl ]
Available Fabric and Vinyl:
Koroseal - Vinyl.
​Guildford of Maine - Fabric.
​Carnegie Xorel - Fabric.
Maharam - Vinyl
Color, Pattern, and Texture: ​​​As selected from manufacturer's full range​​​.
Core: ​​Fiber board​​, [ ​​1/2" inch (13 mm)​​ ] [ 3/8'' inches (9.525 mm) ] thick, laminated to tack surface.
Surface Burning Characteristics: Flame spread index of ​​​25​​​, maximum, and smoke developed index of ​​​450​​​, maximum, when tested in accordance with ASTM E84.
Panel Width: ​​​48 inches (1220 mm)​​​.
Height: ​​​​​​​As indicated on drawings​​​​​​​; No horizontal seams.
Length: As indicated on drawings.
Edge Treatment: Square edge unless detailed otherwise.
Trim: Provide [ Plastic ][ Aluminum ] "J-Mold" type edge trim for exposed edges at door and window openings and similar conditions.
Adhesives: Provide manufacturer's recommended adhesive.
PART 3  EXECUTION
EXAMINATION
Verify that field measurements are as ​indicated​.
Verify that internal wall blocking is ready to receive work and positioning dimensions are as ​indicated on shop drawings​.
PREPARATION
Remove switchplates, wall plates, and surface-mounted fixtures where tackable wall paneling is applied. Reinstall items on completion of installation. [By Others]
Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. [By Others]
INSTALLATION
Install Tack Wall Panels in accordance with manufacturer's instructions.
Secure units level and plumb.
Butt Joints:  Install with tight hairline joints.
Carefully cut holes in boards for ​thermostats​.
Install tackable wall panels in accordance with manufacturer's recommendations on specified substrates with concealed attachments.
Re-wrap top, bottom or side edges for cutting panels around door or window openings, abutting trim, protruding objects, and at other openings, including x-cut at receptacles, light switches, and other openings.
Wrap minimum ​2 inches (51 mm)​ around back of panel.
Carefully cut fiber board, leaving vinyl wallcovering intact.  Wrap wallcovering tightly around edge of board and adhere continuously around back of panel with manufacturer's recommended vinyl wallcovering adhesive.
CLEANING
Clean board surfaces in accordance with manufacturer's instructions.
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